# PComControlActiveX Web Test Program for JavaScript

| PortNo: DSRCheck: CTSCheck: TXBufferSize: RXBufferSize:
common Property | ACKTimer: ResponseTimer: CancelFlag:
Send Data |
ReceiveData |
Polling StxEtxBcc HF UHF Binary Event Status etc1 etc2 Polling common Property APIs
COM/STS: SEN: ERR: ResData:
pcxSendCommandRR
lRecMode lBusyTimeOutms
pcxSendCommand
pcxReceiveResponse
lRecMode lBusyTimeOutms
pcxSendDataRR
lRetryCount
pcxSendData
lACKCheck lRetryCount lStxEtxBcc
pcxReceiveData
lACKResponse lStxEtxBcc
HF Response common Property APIs
Reserve: Resp: Stat: ResDataLen: ResData:
pcxSendDataHFRR
lResponseMode lACKJudge
pcxSendData
lACKCheck lRetryCount lStxEtxBcc
pcxReceiveDataHF
lResponseMode lACKJudge
pcxSendBinaryCommandRR lResponseMode lRetryCount

pcxSendBinaryCommand

lRetryCount

pcxReceiveBinaryReport

lResponseMode lRetryCount

pcxSendBinaryData

pcxReceiveBinaryData

Event Mask

Write Read Mask Value | EVT_PCX_RXCHAR EVT_PCX_TXEMPTY EVT_PCX_ERR_BUFFER_OVERFLOW EVT_PCX_CTS EVT_PCX_DSR EVT_PCX_RLSD | EVT_PCX_BREAK EVT_PCX_RING EVT_PCX_ERR_FRAME EVT_PCX_ERR_OVERRUN EVT_PCX_ERR_PARITY EVT_PCX_ALL

ActiveX Status Block

COM: BaudRate: Databit: Parity: DSRCheck: CTSCheck: Port Claimed: TXBufferSize: RXBufferSize: ACKTimer: ResponseTimer: GetCommStatus: OCXVersion: AutoHandshake: DTRLineControl: RTSLineControl: BreakControl:

COM Port Setting

BaudRate: bps DataBit: bit Parity: AutoHandshake:

DTRLineControl RTSLineControl BreakControl

pcxCharAscHConv

lConvMode: csQconvStr:

pcxDataSumCalc

Sum =

pcxJISconvSJIS

lJConvMode: csQJConvStr:

pcxPrintJobClear

Write Read Dummy Printer List:

LogFlag / LogFileFolder Property

Write Read